
 Digital Multimeter Scope 1.2
 Copyright by METEX Corp. 1994,1995

 Compatibility :
  Hardware requirements : PC 286 or better
  Operating System : MS-DOS 3.10 or later
  Graphics Card : VGA
  Digital Multimeter ( DMM ) compatibility : 

   Family              DMM Models
  ----------------------------------------
   M38xx       :       M3830, M3850
   M36xxCR     :       M3630CR, M3650CR
   M46xxCR     :       M4630CR, M4650CR
   M36xxD      :       M3610D, M3630D, M3640D, M3650D, M3660D

 INSTALLATION
 ==================

 Make a subdirectory on your hard disk for the software.
 For example:    mkdir meter <ENTER>

 Copy the files from the supplied diskette to the subdirectory
 on your hard disk.
 For example:    copy a:\graphic\*.* c:\meter <ENTER>

 SET UP
 ==================

  Connect the Multimeter to your computer's COM Port.
  Make a note of which port ( COM1 or COM2 ) you connect the meter to.

  Turn on the meter.

  Load your computer's mouse driver.

  Start the software by typing 'METEX' and pressing <ENTER>.

  If you do not have a mouse, press F10. The program lets you use
  the arrow and <ENTER> keys to select menu items.
  If you want to use mouse again, press ESC.

 OPERATION NOTES
 =================
 For the NEW and OPEN options on the SHEET menu. Do not enter an
 'extension' for the file name. The software automatically uses :

     '.AUT'     for M3830/50
     '.MNU'     for M36/46CR
     '.3UT'     for M36D

  example)         sample    <ENTER>

 To print an open file, select RUN from the SHEET menu and then press ALT+P.

 The minimum sampling time is 1 sample per second.

 Refer to the HELP menu for a detailed description of each menu.


